|  |  |  |
| --- | --- | --- |
| |  | | --- | | **Software Design Notes** | |  | |
| **FOR EDUCATIONAL USE ONLY** |

|  |
| --- |
| **What is a miniPCB?** |
| A miniPCB is a printed circuit board that contains a layout of an electronic circuit. |
| A miniPCB has a mechanical design that is consistent with numerous similar miniPCBs. |
| A miniPCB has an interface connector that is simple and economical. |
| A miniPCB has educational documentation that is approved by an engineer. |
| A miniPCB is sold in minimum-order-quantities determined by the PCB panel size. |
| [www.minipcb.com](http://www.minipcb.com)  This document is available for free as a download from the GitHub repository: <https://github.com/miniPCB>  This document is associated with the miniPCB Channel on YouTube:  <https://www.youtube.com/@minipcb> |

TABLE OF CONTENTS

[Introduction 4](#_Toc129543724)

[Specification Requirements 5](#_Toc129543725)

[Source Code 11](#_Toc129543726)

[Firmware Release History 12](#_Toc129543727)

[Change and Liability Notice 13](#_Toc129543728)

[Trademark Notice 13](#_Toc129543729)

[Revision History 13](#_Toc129543730)

[Related Content 14](#_Toc129543731)

TABLE OF FIGURES

**TABLE OF TABLES**

[Table 1 – \FilePath\FileName1.ext 11](#_Toc130071942)

[Table 2 – \FilePath\FileName2.ext 11](#_Toc130071943)

[Table 3 – \FilePath\FileName3.ext 11](#_Toc130071944)

[Table 4 – \FilePath\FileName4.ext 11](#_Toc130071945)

[Table 5 – Release 000-000-0-NM.DDMMMYYYY 12](#_Toc130071946)

# Introduction

## Purpose

The purpose of this document is to record software design notes for the 13A-777 miniPCB.

## Scope

The scope of this document is limited to specifications and requirements, source code, and firmware releases.

## File Locations

|  |  |
| --- | --- |
| **FILE NAME** | **FILE LOCATION** |
| [ALL] | https://github.com/miniPCB/EAGLE/tree/main/miniPCB/13/A/13A-777 |

## Definitions and Abbreviations

* Convitae, the ratio of a response per input behavior.
* DHM, device histogram matrix, used to organize and access data.
* HPC, histogram program counter, used to track most recent game.
* HVC, histogram vector counter, used to track most recent entry.

# Specification Requirements

#### SSR1 – Hardware Abstraction

No text (title)

#### SSR1.1 – Power

Manage power with these functional modes:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| sleepDeep | Minimal power consumption mode. |
| sleepActive | Low power consumption mode without sleeping. |
| activeGame | High power consumption mode. |
| batteryVoltage | Reads the current battery voltage. |

#### SSR1.2 – LCD

Control the 2x16 LCD with these functions:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| setContrast | Controls the voltage controlling the LCD contrast. |
| setBacklight | Controls the voltage controlling the LCD backlight. |
| refreshScreen | Writes the full screen to the LCD module. |

#### SSR1.3 – LED

Control the LED indicator with these functions:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| setLED | Turns an LED indicator on. |
| clearLED | Turns an LED indicator off. |
| toggleLED | Toggles an LED indicator from off to on, or on to off. |

#### SSR1.4 – Primary Select Button

Interface with the primary select button with this function:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| readSelectButton | Signals include: (1) wake, (2) confirm, (3) select. |

#### SSR1.5 – Rotary Encoder

Interface with a rotary encoder with these functions:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| setEncoderRGB | Sets color of the RGB LED on the encoder. |
| readEncoderButton | Reads the encoder button switch. |
| readEncoderRotation | Reads the encoder rotation count. |

#### SSR1.6 – Device Clock

Maintain a device clock with 1 second resolution with these functions:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| setTimer | Sets value in timer counter. |
| getTimer | Reads value in timer counter. |
| incTimer | Increments value in timer counter. |
| spareTime | Returns with the counts available in the long (8 bytes). |
| timerRatio | Returns with the ratio of current\_count per max\_count. |

#### SSR1.7 – Device Histogram

No text (title)

#### SSR1.7.1 – Histogram Programming Interface

Maintain a device histogram with these functions:

|  |  |
| --- | --- |
| **FUNCTION** | **DESCRIPTION** |
| writeHistogram | Adds a new record to the device histogram.  Clears user interaction counters: buttonpress, encoderpress, and rotation. |
| writeHistogramValue | Writes a value to a device histogram. |
| playHistogram | Moves each value of the device histogram through the working register. |
| readHistorgram | Reads the histogram matrix. |
| readHistogramValue | Reads a value from the histogram matrix. |

#### SSR1.7.2 – Game Results

Memory available for recording whatever game result is available.

#### SSR1.7.3 – Count Ratios

Device count ratios are computed by dividing a count-value by the max-count-value.

#### SSR1.7.4 – Rolling Memory

Write over the oldest data in the matrix to accommodate new data.

#### SSR1.7.5 – Histogram Program Counter (HPC)

Use a histogram counter to keep track of the most recent histogram entry.

#### SSR1.7.6 – Histogram Vector Counter (HVC)

Use a histogram counter to keep track of the most recent vector entry.

#### SSR1.7.7 – Device Histogram Matrix (DHM)

Use the histogram counters to form a matrix.

#### SSR1.7.8 – Histogram Vector

Device histogram will be comprised of a matrix of vectors defined below.

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **DATA NAME** | **TYPE** | **INTUITIVE FOCUS** |
| **0** | GAME RESULT 0 | char | GAME CONVITAE \* USER CONVITAE |
| **1** | GAME RESULT 1 | char |
| **2** | GAME RESULT 3 | char |
| **3** | GAME RESULT 4 | char |
| **4** | GAME RESULT 5 | char |
| **5** | GAME RESULT 6 | char |
| **6** | GAME RESULT 7 | char |
| **7** | GAME RESULT 8 | char |
| **8** | SECOND COUNT RATIO | char | DEVICE CONVITAE |
| **9** | BUTTONPRESS COUNT RATIO | char |
| **A** | ROTATION COUNT RATIO | char |
| **B** | ENCODERPRESS COUNT RATIO | char |
| **C** | BATTERY VOLTAGE RATIO | char |
| **D** | USER SIGNAL 0 (LIVE) | char | DEVICE CONVITAE \* USER CONVITAE |
| **E** | USER SIGNAL 1 (LOVE) | char |
| **F** | USER SIGNAL 2 (LEARN) | char |

#### SSR1.7.9 – Histogram Memory Map

Device histogram will be mapped according to the memory map defined below.

|  |  |  |  |
| --- | --- | --- | --- |
| **#** | **HPC** | **HVC = 0**  **MEMORY ADDRESS** | **HVC = 15**  **MEMORY ADDRESS** |
| **0** | 0 | 2A0h | 2AFh |
| **1** | 1 | 2B0h | 2BFh |
| **2** | 2 | 2C0h | 2CFh |
| **3** | 3 | 2D0h | 2DFh |
| **4** | 4 | 2E0h | 2EFh |
| **5** | 5 | 320h | 32Fh |
| **6** | 6 | 330h | 33Fh |
| **7** | 7 | 340h | 34Fh |
| **8** | 8 | 350h | 35Fh |
| **9** | 9 | 360h | 36Fh |
| **10** | 10 | 3A0h | 3AFh |
| **11** | 11 | 3B0h | 3BFh |
| **12** | 12 | 3C0h | 3CFh |
| **13** | 13 | 3D0h | 3DFh |
| **14** | 14 | 3E0h | 3EFh |

#### SSR2 – Toy Functionality

No text (title)

#### SSR2.1 – Sleep

The device will enter a low power mode when not in use.

#### SSR2.2 – Wakeup

The device will wake from low power mode when the Primary Select Button is pressed.

#### SSR2.3 – Sleep

Selects catalog entries according to three variables: (1) the user control of the button input, (2) the game being played, and (3) the state of game being played.

#### SSR2.4 – Sleep

Selects catalog entries according to three variables: (1) the user control of the button input, (2) the game being played, and (3) the state of game being played.

#### SSR3 – Game Functionality

No text (title)

#### SSR3.1 – Sleep

Selects catalog entries according to three variables: (1) the user control of the button input, (2) the game being played, and (3) the state of game being played.

# Source Code

Table – \FilePath\FileName1.ext

|  |
| --- |
| INSERT CODE HERE |

Table – \FilePath\FileName2.ext

|  |
| --- |
| INSERT CODE HERE |

Table – \FilePath\FileName3.ext

|  |
| --- |
| INSERT CODE HERE |

Table – \FilePath\FileName4.ext

|  |
| --- |
| INSERT CODE HERE |

# Firmware Release History

Table – Release 000-000-0-NM.DDMMMYYYY

|  |  |
| --- | --- |
| **File Name** |  |
| **File Size** |  |
| **File Location** |  |
| **Target Hardware** |  |
| **Maturity Level** |  |
| **Compiler Notes** |  |

# Change and Liability Notice

This document is subject to change without notice. While effort has been made to ensure the accuracy of the material contained within this document, Nolan Manteufel shall under no circumstances be liable for incidental or consequential damages or related expenses resulting from the use of this document.

# Trademark Notice

miniPCB is a trademark of Nolan Manteufel.

This document does not constitute permission to use the miniPCB trademark.

|  |  |  |
| --- | --- | --- |
| WORDMARK | FIGUREMARK | FIGUREMARK |
| miniPCB™ | A picture containing drawing  Description automatically generated™ | Icon  Description automatically generated™ |

# Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| REV | DESCRIPTION | ECO | DATE |
| A | Initial Release | N/A | DDMMMYYYY |
|  |  |  |  |

# Related Content

|  |  |  |  |
| --- | --- | --- | --- |
| # | TYPE | DESCRIPTION | LOCATION |
| 1 | Sale Posting | eBay |  |
| 2 | Sale Posting | Mouser |  |
| 3 | Repository | Engineering Files | https://github.com/miniPCB/EAGLE/tree/main/miniPCB/13/A/13A-777 |
| 4 | Video | Preparation | https://youtu.be/YeX36dg0lwk |
| 5 | Video | Design | https://youtu.be/6YcOx\_vTpKk |
| 6 | Video | Documentation | https://youtu.be/-dhOiV1X4uM |
| 7 | Video | Development |  |
| 8 | Video | Testing |  |
|  | Video | Engineering Release |  |