|  |  |  |  |
| --- | --- | --- | --- |
| **TEST IDENTIFICATION** | | | |
| **TEST NAME** | | | |
| Capacitance Value, C3 | | | |
| **TEST NO\*** | T10 | **UUT PN** | 04A-005 |
| **LAST TEST NO** | T9 | **TEST TYPE** | STATIC |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **COMPONENTS UNDER TEST** | | | | |
| **REF DES** | **TYPE** | **PARAMETER** | **FAILURE MODE** | **TEST LIMIT** |
| C3 | CAPACITOR (GENERAL) | CAPACITANCE | Out of Tolerance: HIGH | UPPER |
| Out of Tolerance: LOW | LOWER |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |
|  | N/A | N/A | N/A | N/A |
| N/A | N/A |

|  |
| --- |
| **TEST PROCEDURE** |
| **PURPOSE** |
| Verify capacitor is within expected resistance tolerance. |
| **SCOPE** |
| Handheld multimeter measurement at test points. |
|  |
| N/A |

|  |  |  |  |
| --- | --- | --- | --- |
| **POWER** | | | |
| None | | | |
| **STIMULI** | | | |
| None | | | |
| **MEASUREMENT** | | | |
| Measure capacitance across capacitor. | | | |
| **SIGNAL PIN** | TP5 |  | |
|  | | |  |
| **RETURN PIN** | TP10 |  | |
|  | | |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ACCEPTANCE CRITERIA** | | | | |
| **PARAMETER** | **LOWER LIMIT** | **TARGET VALUE** | **UPPER LIMIT** | **UNITS** |
| CAPACITANCE | 42.3 nF | 47 nF | 51.7 nF | FARADS |

|  |  |  |  |
| --- | --- | --- | --- |
| **TEST RESULTS** | | | |
| **RESULT** | **NEXT STEP** | **ADJUST** | **REPLACE** |
| IN TOLERANCE | T11 | N/A | N/A |
| OOT HIGH | END FAIL | N/A | C3 |
| OOT LOW | END FAIL | N/A | C3 |
| OOT HIGH AND UNABLE TO ADJUST | N/A | N/A | N/A |
| OOT LOW AND UNABLE TO ADJUST | N/A | N/A | N/A |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **This Space Intentionally Blank** | | | | |
| **Form Controls** | | | | |
|  | |  |  |  |
| Log Entry Key | 20230205193841 | | | |
| Computer ID |  | | | |
| User ID |  | | | |
| Date Time |  | | | |
| PDF |  | | | |